# VGA Simulator

Log File:
Resolution X: Resolution Y: Pixel Clock Rate (MHz):
Back Porch X:
Back Porch Y:
Click on frames to review:
Download current frame
Log file guidelines:

- Must be a .txt file
- The .txt file lines should be formatted as so:
  `current_sim_time time_units: hs vs red green blue`
  ex. `535 ns: 1 1 010 010 01`
- Everything should be binary except sim time
- Pad red, green, and blue with `0` (zeroes) to the max color depth
- Log a line every rising edge of a clock that is synchronized with your pixel clock and is just as fast or oversamples.
- Make sure you set your clock period correctly in your testbench!